{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Readme","Sheet3","Sheet4"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Readme","index":0,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"エマグラムをExcel VBAを利用して描く"]
[]
[]
[null,null,"簡単な使い方"]
[]
[null,null,"１．Sheet4を開く"]
[null,null,"２．すでにエマグラムが描画されていたら、マクロから”すべてを選択”を実行し、選択されたら、DELキーで消去する"]
[null,null,"３．マクロから”エマグラム描画”を実行、ダイアログの各タブ毎の入力データを確認、変更する"]
[null,null,"４．ダイアログの”OK\"ボタンでエマグラムをSheet4上に描画する。”Cancel”で取消する。"]
[]
[null,null,"注１：　エマグラムを描画するシートは何処でも構わない。Sheet3上でマクロ”エマグラム描画”を実行すると、Sheet3に描画される。"]
[null,null,"注２：　エマグラムの描画は、短い線分の集合です。全体を移動させるときなど、これら線分をグループ化しておくと容易です。"]

{"sheet":"Sheet3","index":1,"n_rows":92,"n_cols":13,"rows_kept":92,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,"47678 Hachijyojima Observations at 00Z 14 Jul 2015"]
[]
[]
[null,null,"PRES","HGHT","TEMP","DWPT","RELH","MIXR","DRCT","SKNT","THTA","THTE","THTV"]
[null,null,"hPa","m","C","C","%","g/kg","deg","knot","K","K","K"]
[]
[null,null,1000,92]
[null,null,993,153,27.4,24.3,83,19.71,205,11,301.10000000000002,359.5,304.7]
[null,null,992,162,25.6,22.3,82,17.420000000000002,205,11,299.39999999999998,350.5,302.60000000000002]
[null,null,959,459,23.5,20.3,82,15.92,220,17,300.2,347,303.10000000000002]
[null,null,925,775,21.2,18.2,83,14.43,210,16,301,343.6,303.60000000000002]
[null,null,917,850,21,17,78,13.47,208,16,301.5,341.4,304]
[null,null,901,1003,21,11,53,9.23,204,15,303,330.8,304.7]
[null,null,850,1506,19.2,11.2,60,9.92,190,12,306.2,336.4,308.10000000000002]
[null,null,842,1587,18.8,8.8000000000000007,52,8.51,188,12,306.60000000000002,332.7,308.2]
[null,null,818,1832,17,7.6,54,8.09,180,10,307.3,332.2,308.8]
[null,null,784,2190,14.4,5.9,57,7.49,205,8,308.3,331.5,309.7]
[null,null,729,2805,10,3,62,6.56,167,11,309.89999999999998,330.4,311.10000000000002]
[null,null,719,2920,9.8000000000000007,-0.6,49,5.14,160,12,310.89999999999998,327.2,311.8]
[null,null,705,3083,9.4,-5.6,34,3.59,156,13,312.2,323.89999999999998,312.89999999999998]
[null,null,700,3142,9.1999999999999993,-5.8,34,3.56,155,14,312.60000000000002,324.2,313.3]
[null,null,663,3590,7.9,-14.7,19,1.86,175,17,316,322.39999999999998,316.39999999999998]
[null,null,656,3677,7.6,-16.399999999999999,16,1.63,173,16,316.7,322.3,317]
[null,null,614,4220,5.8,-14.2,22,2.09,162,13,320.7,327.9,321.10000000000002]
[null,null,606,4326,5.2,-15.3,21,1.93,160,12,321.2,327.9,321.60000000000002]
[null,null,578,4708,3.2,-19.2,17,1.45,160,8,323.2,328.4,323.5]
[null,null,555,5037,1.4,-22.6,15,1.1299999999999999,145,12,324.89999999999998,329,325.10000000000002]
[null,null,542,5229,0.4,-24.6,13,0.97,167,9,325.89999999999998,329.4,326.10000000000002]
[null,null,532,5377,-0.4,-27.3,11,0.77,185,6,326.60000000000002,329.5,326.8]
[null,null,500,5870,-3.1,-36.1,6,0.35,160,12,329.2,330.6,329.3]
[null,null,487,6078,-4.3,-31.7,10,0.55000000000000004,160,14,330.2,332.3,330.3]
[null,null,477,6242,-5.3,-28.3,15,0.78,155,15,330.9,333.9,331.1]
[null,null,449,6716,-7.9,-31.9,13,0.59,140,17,333.4,335.7,333.6]
[null,null,419,7253,-10.3,-25.3,28,1.17,123,20,337,341.5,337.2]
[null,null,405,7514,-11.5,-25.7,30,1.17,115,21,338.8,343.2,339]
[null,null,400,7610,-11.9,-25.9,30,1.1599999999999999,120,23,339.4,343.9,339.7]
[null,null,366,8271,-16.8,-31.6,27,0.75,115,19,341.6,344.6,341.7]
[null,null,348,8646,-19.600000000000001,-34.799999999999997,25,0.57999999999999996,130,21,342.8,345.1,342.9]
[null,null,312,9458,-25.7,-41.7,21,0.32,126,24,345.2,346.5,345.2]
[null,null,300,9740,-28.3,-42.3,25,0.31,125,25,345.4,346.7,345.4]
[null,null,250,11020,-39.1,-48.1,38,0.2,120,35,347.8,348.6,347.8]
[null,null,249,11047,-39.4,-48.4,38,0.19,120,35,347.8,348.7,347.9]
[null,null,246,11130,-40.1,-49.1,38,0.18,119,35,347.9,348.7,347.9]
[null,null,200,12510,-51.1,null,null,null,105,35,351.7,null,351.7]
[null,null,150,14320,-65.099999999999994,null,null,null,90,33,357.7,null,357.7]
[null,null,139,14781,-68.099999999999994,null,null,null,90,31,360.3,null,360.3]
[null,null,136,14910,-68.599999999999994,null,null,null,90,31,361.6,null,361.6]
[null,null,120,15650,-71.7,null,null,null,105,27,369.2,null,369.2]
[null,null,107,16328,-74.5,null,null,null,61,24,376.2,null,376.2]
[null,null,104,16493,-75,null,null,null,50,23,378.3,null,378.3]
[null,null,100,16720,-75.7,null,null,null,70,27,381.2,null,381.2]
[null,null,97.9,16842,-75.900000000000006,null,null,null,75,31,383.1,null,383.1]
[null,null,70,18820,-65.900000000000006,null,null,null,85,21,443.1,null,443.1]
[null,null,50,20890,-60.9,null,null,null,95,23,499.5,null,499.5]
[null,null,30,24100,-56.3,null,null,null,85,31,590.6,null,590.6]
[null,null,20,26750,-46.5,null,null,null,110,37,693.1,null,693.1]
[null,null,11.4,30505,-38.4,null,null,null,85,74,842.9,null,842.9]
[null,null,10,31380,-36.5,null,null,null,100,41,882.1,null,882.1]
[]
[null,null,"Station information and sounding indices"]
[]
[null,null,"Station number:",47678]
[null,null,"Observation time:","150714/0000"]
[null,null,"Station latitude:",33.11]
[null,null,"Station longitude:",139.78]
[null,null,"Station elevation:",153]
[null,null,"Showalter index:",5.31]
[null,null,"Lifted index:",0.79]
[null,null,"LIFT computed using virtual temperature:",-0.09]
[null,null,"SWEAT index:",170.41]
[null,null,"K index:",18.5]
[null,null,"Cross totals index:",14.3]
[null,null,"Vertical totals index:",22.3]
[null,null,"Totals totals index:",36.6]
[null,null,"Convective Available Potential Energy:",27.1]
[null,null,"CAPE using virtual temperature:",103.76]
[null,null,"Convective Inhibition:",-77.97]
[null,null,"CINS using virtual temperature:",-34.78]
[null,null,"Equilibrum Level:",668.93]
[null,null,"Equilibrum Level using virtual temperature:",475.92]
[null,null,"Level of Free Convection:",772.78]
[null,null,"LFCT using virtual temperature:",805.25]
[null,null,"Bulk Richardson Number:",3.03]
[null,null,"Bulk Richardson Number using CAPV:",11.6]
[null,null,"Temp [K] of the Lifted Condensation Level:",293.11]
[null,null,"Pres [hPa] of the Lifted Condensation Level:",921.4]
[null,null,"Mean mixed layer potential temperature:",300.06]
[null,null,"Mean mixed layer mixing ratio:",16.239999999999998]
[null,null,"1000 hPa to 500 hPa thickness:",5778]
[null,null,"Precipitable water [mm] for entire sounding:",34.770000000000003]

{"sheet":"Sheet4","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}